**Bilaga 1**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Riskgrupp | 1.1 -1.2  1.3-1.4  1.5-1.6 | 1.4S | 2.1 | 2.2 | 2.3 | 3 | 4.1 | 4.2 | 4.3 | 5.1 | 5.2 | 6.1 | 6.2 | 7  A/BIC | 8 | 9 | 9A |
| 1.1 -1.2  1.3-1.4  1.5-1.6 | ***För klass 1 se tabell 2*** | | s | s | s | s | s | s | s | s | s | s | s | s | s | s | s |
| 1.4S |  | + | + | + | + | + | + | + | + | + | + | + | + | + | + | + | + |
| 2.1 | s | + | + | + | + | + | s | + | + | s | s | + | + | + | + | + | s |
| 2.2 | s | + | + | + | + | + | s | + | + | + | s | + | + | + | + | + | + |
| 2.3 | s | + | + | + | + | + | s | + | + | + | s | + | + | + | + | + | + |
| 3 | s | + | + | + | + | + | s | + | + | s | s | + | + | + | + | + | s |
| 4.1 | s | + | s | s | s | s | + | s | s | s | s | s | s | s | s | s | s |
| 4.2 | s | + | + | + | + | + | s | + | + | s | s | + | + | + | + | + | s |
| 4.3 | s | + | + | + | + | + | s | + | + | s | s | + | + | + | s | + | s |
| 5.1 | s | + | s | + | + | s | s | s | s | + | s | + | + | + | s | + | s |
| 5.2 | s | + | s | s | s | s | s | s | s | s | + | s | s | s | s | s | s |
| 6.1 | s | + | + | + | + | + | s | + | + | + | s | + | + | + | IX] | + | + |
| 6.2 | s | + | + | + | + | + | s | + | + | + | s | + | + | + | + | + | + |
| 7 A/BIC | s | + | + | + | + | + | s | + | + | + | s | + | + | + | + | + | + |
| 8 | s | + | + | + | + | + | s | + | s | s | s | IX] | + | + | IX] | + | + |
| 9 | s | + | + | + | + | + | s | + | + | + | s | + | + | + | + | + | + |
| **9A** | s | + | s | + | + | s | s | s | s | s | s | + | + | + | + | + | + |

Tabell 1. Krav på samlastning och lastseparering

Tabellförklaringar:

+ förpackningar kan transporteras utan att separeras

S förpackningar måste separeras från varandra på ett avstånd av minst 2 m i varje riktning

förpackningarnas kompatibilitet ska kontrolleras separat

XX

För klass 8

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CG** | **A** | **B** | **C** | **D** | **E** | **F** | **G** | **H** | **J** | **K** | **L** | **N** | **S** |
| **A** |  | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **** | **S** | **S** |
| **B** | **S** |  | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **** | **S** |  |
| **C** | **S** | **S** |  |  |  | **S** |  | **S** | **S** | **S** | **** | **S** |  |
| **D** | **S** | **S** |  |  |  | **S** |  | **S** | **S** | **S** | **** | **S** |  |
| **E** | **S** | **S** |  |  |  | **S** |  | **S** | **S** | **S** | **** | **S** |  |
| **F** | **S** | **S** | **S** | **S** | **S** |  | **S** | **S** | **S** | **S** | **** | **S** |  |
| **G** | **S** | **S** |  |  |  | **S** |  | **S** | **S** | **S** | **** | **S** |  |
| **H** | **S** | **S** | **S** | **S** | **S** | **S** | **S** |  | **S** | **S** | **** | **S** |  |
| **J** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** |  | **S** | **** | **S** |  |
| **K** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** |  | **** | **S** |  |
| **L** | **** | **** | **** | **** | **** | **** | **** | **** | **** | **** |  | **** | **** |
| **N** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **S** | **** |  |  |
| **S** | **S** |  |  |  |  |  |  |  |  |  | **** |  |  |

Tabell 2. Krav på samlastning och lastseparering av förpackningar i riskgrupp 1

Tabellförklaringar:

 förpackningar kan transporteras utan att separeras

S förpackningar måste separeras från varandra på ett avstånd av minst 2 m i varje riktning

förpackningarnas kompatibilitet ska kontrolleras separat

XX

• if at least one item (within CG C, D, E and G) is a SRD-6.6 DG, the packages must be separated by at least 2 m in any direction;

if both items (within CG C, D, E and G) are IATA DG, the packages are compatible and may be carried without separation;

CG L articles may only be carried on the same aircraft with the same type of explosives in CG L and cannot be carried with any other DG

förpackningar får inte transporteras i samma luftfartyg